**Assignment -4**

|  |  |
| --- | --- |
| Assignment Date | 08 October 2022 |
| Student Name | S. Gobika |
| Student Roll Number | 820319106007 |
| Maximum Marks | 2 Marks |

# Question:

Write code and connections in wokwi for the ultrasonic sensor.

Whenever the distance is less than 100 cms send an "alert" to the IBM cloud and display in the device recent events.

# Code:

#define trigPin 12

#define echoPin 13

int Buzzer = 8; // Connect buzzer pin to 8 int ledPin= 6; //Connect LEd pin to 6

int duration, distance; //to measure the distance and time taken

void setup() {

Serial.begin (9600);

//Define the output and input objects(devices) pinMode(trigPin, OUTPUT); pinMode(echoPin, INPUT); pinMode(Buzzer, OUTPUT); pinMode(ledPin, OUTPUT);

}

void loop() {

digitalWrite(trigPin, HIGH); delayMicroseconds(10); digitalWrite(trigPin, LOW); duration = pulseIn(echoPin, HIGH); distance = (duration/2) / 29.1;

//when distance is greater than or equal to 200 OR less than or equal to 0,the buzzer and LED are off

if (distance >= 200 || distance <= 0)

{

Serial.println("no object detected"); digitalWrite(Buzzer,LOW);

digitalWrite(ledPin,LOW);

}

else {

Serial.println("object detected \n"); Serial.print("distance= ");

Serial.print(distance); //prints the distance if it is between the range 0 to 200 tone(Buzzer,400); // play tone of 400Hz for 500 ms digitalWrite(ledPin,HIGH);

}

}

# Screenshot (4).pngOutput: